KERN: PCI:   interrupt_line 0b, interrupt_pin 01
KERN: PCI:   ROM base host 00000000, pci 00000000, size ??
KERN: PCI:   base reg 0: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 1: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: PM, PCIe, MSI, subvendor, HyperTransport
KERN: PCI:   Extended capabilities: Vendor Unique, Virtual Channel
KERN: PCI: [dom 0, bus  0] bus   0, device 17, function  0: vendor 1002, device 4390, revision 00
KERN: PCI:   class_base 01, class_function 01, class_api 8f
KERN: PCI:   vendor 1002: Advanced Micro Devices, Inc. [AMD/ATI]
KERN: PCI:   device 4390: SB7x0/SB8x0/SB9x0 SATA Controller [IDE mode]
KERN: PCI:   info: Mass storage controller (IDE interface, PCI native mode control
KERN: PCI:   line_size 00, latency 40, header_type 00, BIST 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size 00000000
KERN: PCI:   cardbus_CIS 00000000, subsystem_id 021a, subsystem_vendor_id 1025
KERN: PCI:   interrupt_line 0b, interrupt_pin 01, min_grant 00, max_latency 00
KERN: PCI:   base reg 0: host 00008420, pci 00008420, size 00000008, flags 01
KERN: PCI:   base reg 1: host 00008414, pci 00008414, size 00000004, flags 01
KERN: PCI:   base reg 2: host 00008418, pci 00008418, size 00000008, flags 01
KERN: PCI:   base reg 3: host 00008410, pci 00008410, size 00000004, flags 01
KERN: PCI:   base reg 4: host 00008400, pci 00008400, size 00000010, flags 01
KERN: PCI:   base reg 5: host f0207000, pci f0207000, size 00000400, flags 00
KERN: PCI:   Capabilities: PM, SATA
KERN: PCI: [dom 0, bus  0] bus   0, device 18, function  0: vendor 1002, device 4397, revision 00
KERN: PCI:   class_base 0c, class_function 03, class_api 10
KERN: PCI:   vendor 1002: Advanced Micro Devices, Inc. [AMD/ATI]
KERN: PCI:   device 4397: SB7x0/SB8x0/SB9x0 USB OHCI0 Controller
KERN: PCI:   info: Serial bus controller (USB controller, OHCI)
KERN: PCI:   line_size 08, latency 40, header_type 80, BIST 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size 00000000
KERN: PCI:   cardbus_CIS 00000000, subsystem_id 021a, subsystem_vendor_id 1025
KERN: PCI:   interrupt_line 0a, interrupt_pin 01, min_grant 00, max_latency 00
KERN: PCI:   base reg 0: host f0004000, pci f0004000, size 00001000, fKERN: lags 00
KERN: PCI:   base reg 1: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 2: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 3: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 4: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 5: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: (not supported)
KERN: PCI: [dom 0, bus  0] bus   0, device 18, function  1: vendor 1002, device 4398, revision 00
KERN: PCI:   class_base 0c, class_function 03, class_api 10
KERN: PCI:   vendor 1002: Advanced Micro Devices, Inc. [AMD/ATI]
KERN: PCI:   device 4398: SB7x0 USB OHCI1 Controller
KERN: PCI:   info: Serial bus controller (USB controller, OHCI)
KERN: PCI:   line_size 08, latency 40, header_type 00, BIST 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size 00000000
KERN: PCI:   cardbus_CIS 00000000, subsystem_id 021a, subsystem_vendor_id 1025
KERN: PCI:   interrupt_line 0a, interrupt_pin 01, min_grant 00, max_latency 00
KERN: PCI:   base reg 0: host f0005000, pci f0005000, size 00001000, flags 00
KERN: PCI:   base reg 1: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 2: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 3: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 4: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 5: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: (not supported)
KERN: PCI: [dom 0, bus  0] bus   0, device 18, function  2: vendor 1002, device 4396, revision 00
KERN: PCI:   class_base 0c, class_function 03, class_api 20
KERN: PCI:   vendor 1002: Advanced Micro Devices, Inc. [AMD/ATI]
KERN: PCI:   device 4396: SB7x0/SB8x0/SB9x0 USB EHCI Controller
KERN: PCI:   info: Serial bus controller (USB controller, EHCI)
KERN: PCI:   line_size 08, latency 40, header_type 00, BIST 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size 00000000
KERN: PCI:   cardbus_CIS 00000000, subsystem_id 021a, subsystem_vendor_id 1025
KERN: PCI:   interrupt_line 05, interrupt_pin 02, min_grant 00, max_latency 00
KERN: PCI:   base reg 0: host f0207400, pci f0207400, size 00000100, flags 00
KERN: PCI:   base reg 1: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 2: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 3: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 4: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 5: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: PM, DebugPort
KERN: PCI: [dom 0, bus  0] bus   0, device 19, function  0: vendor 1002, device 4397, revision 00
KERN: PCI:   class_base 0c, class_function 03, class_api 10
KERN: PCI:   vendor 1002: Advanced Micro Devices, Inc. [AMD/ATI]
KERN: PCI:   device 4397: SB7x0/SB8x0/SB9x0 USB OHCI0 Controller
KERN: PCI:   info: Serial bus controller (USB controller, OHCI)
KERN: PCI:   line_size 08, latency 40, header_type 80, BIST 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size 00000000
KERN: PCI:   cardbus_CIS 00000000, subsystem_id 021a, subsystem_vendor_id 1025
KERN: PCI:   interrupt_line 0b, interrupt_pin 01, min_grant 00, max_latency 00
KERN: PCI:   base reg 0: host f0006000, pci f0006000, size 00001000, flags 00
KERN: PCI:   base reg 1: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 2: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 3: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 4: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 5: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: (not supported)
KERN: PCI: [dom 0, bus  0] bus   0, device 19, function  2: vendor 1002, device 4396, revision 00
KERN: PCI:   class_base 0c, class_function 03, class_api 20
KERN: PCI:   vendor 1002: Advanced Micro Devices, Inc. [AMD/ATI]
KERN: PCI:   device 4396: SB7x0/SB8x0/SB9x0 USB EHCI Controller
KERN: PCI:   info: Serial bus controller (USB controller, EHCI)
KERN: PCI:   line_size 08, latency 40, header_type 00, BIST 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size 00000000
KERN: PCI:   cardbus_CIS 00000000, subsystem_id 021a, subsystem_vendor_id 1025
KERN: PCI:   interrupt_line 0b, interrupt_pin 02, min_grant 00, max_latency 00
KERN: PCI:   base reg 0: host f0207800, pci f0207800, size 00000100, flags 00
KERN: PCI:   base reg 1: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 2: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 3: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 4: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 5: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: PM, DebugPort
KERN: PCI: [dom 0, bus  0] bus   0, device 20, function  0: vendor 1002, device 4385, revision 3a
KERN: PCI:   class_base 0c, class_function 05, class_api 00
KERN: PCI:   vendor 1002: Advanced Micro Devices, Inc. [AMD/ATI]
KERN: PCI:   device 4385: SBx00 SMBus Controller
KERN: PCI:   info: Serial bus controller (SMBus)
KERN: PCI:   line_size 00, latency 00, header_type 80, BIST 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size 00000000
KERN: PCI:   cardbus_CIS 00000000, subsystem_id 021a, subsystem_vendor_id 1025
KERN: PCI:   interrupt_line 00, interrupt_pin 00, min_grant 00, max_latency 00
KERN: PCI:   base reg 0: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 1: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 2: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 3: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 4: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 5: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: HyperTransport
KERN: PCI: [dom 0, bus  0] bus   0, device 20, function  2: vendor 1002, device 4383, revision 00
KERN: PCI:   class_base 04, class_function 03, class_api 00
KERN: PCI:   vendor 1002: Advanced Micro Devices, Inc. [AMD/ATI]
KERN: PCI:   device 4383: SBx00 Azalia (Intel HDA)
KERN: PCI:   info: Multimedia controller (Audio device)
KERN: PCI:   line_size 08, latency 40, header_type 00, BIST 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size 00000000
KERN: PCI:   cardbus_CIS 00000000, subsystem_id 021a, subsystem_vendor_id 1025
KERN: PCI:   interrupt_line 0a, interrupt_pin 01, min_grant 00, max_latency 00
KERN: PCI:   base reg 0: host 00000000f0000000, pci 00000000f0000000, size 00004000, flags 04 00
KERN: PCI:   base reg 2: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 3: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 4: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 5: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: PM
KERN: PCI: [dom 0, bus  0] bus   0, device 20, function  3: vendor 1002, device 439d, revision 00
KERN: PCI:   class_base 06, class_function 01, class_api 00
KERN: PCI:   vendor 1002: Advanced Micro Devices, Inc. [AMD/ATI]
KERN: PCI:   device 439d: SB7x0/SB8x0/SB9x0 LPC host controller
KERN: PCI:   info: Bridge (ISA bridge)
KERN: PCI:   line_size 00, latency 00, header_type 80, BIST 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size 00000000
KERN: PCI:   cardbus_CIS 00000000, subsystem_id 021a, subsystem_vendor_id 1025
KERN: PCI:   interrupt_line 00, interrupt_pin 00, min_grant 00, max_latency 00
KERN: PCI:   base reg 0: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 1: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 2: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 3: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 4: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 5: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: (not supported)
KERN: PCI: [dom 0, bus  0] bus   0, device 20, function  4: vendor 1002, device 4384, revision 00
KERN: PCI:   class_base 06, class_function 04, class_api 01
KERN: PCI:   vendor 1002: Advanced Micro Devices, Inc. [AMD/ATI]
KERN: PCI:   device 4384: SBx00 PCI to PCI Bridge
KERN: PCI:   info: Bridge (PCI bridge, Subtractive decode)
KERN: PCI:   line_size 00, latency 40, header_type 81, BIST 00
KERN: PCI:   subsystem_id 0000, subsystem_vendor_id 0000
KERN: PCI:   primary_bus 00, secondary_bus 0f, subordinate_bus 0f, secondary_latency 40
KERN: PCI:   I/O window 0000-0fff
KERN: PCI:KERN:    memory window 00000000-000fffff
KERN: PCI:   prefetchable memory window 0000000000000000-00000000000fffff
KERN: PCI:   bridge_control 0823, secondary_status 0280
KERN: PCI:   interrupt_line 00, interrupt_pin 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size ??
KERN: PCI:   base reg 0: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 1: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: (not supported)
KERN: PCI: [dom 0, bus  0] bus   0, device 24, function  0: vendor 1022, device 1300, revision 40
KERN: PCI:   class_base 06, class_function 00, class_api 00
KERN: PCI:   vendor 1022: Advanced Micro Devices, Inc. [AMD]
KERN: PCI:   device 1300: Family 11h Processor HyperTransport Configuration
KERN: PCI:   info: Bridge (Host bridge)
KERN: PCI:   line_size 00, latency 00, header_type 80, BIST 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size 00000000
KERN: PCI:   cardbus_CIS 00000000, subsystem_id 0000, subsystem_vendor_id 0000
KERN: PCI:   interrupt_line 00, interrupt_pin 00, min_grant 00, max_latency 00
KERN: PCI:   base reg 0: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 1: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 2: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 3: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 4: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 5: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: HyperTransport
KERN: PCI: [dom 0, bus  0] bus   0, device 24, function  1: vendor 1022, device 1301, revision 00
KERN: PCI:   class_base 06, class_function 00, class_api 00
KERN: PCI:   vendor 1022: Advanced Micro Devices, Inc. [AMD]
KERN: PCI:   device 1301: Family 11h Processor Address Map
KERN: PCI:   info: Bridge (Host bridge)
KERN: PCI:   line_size 00, latency 00, header_type 80, BIST 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size 00000000
KERN: PCI:   cardbus_CIS 00000000, subsystem_id 0000, subsystem_vendor_id 0000
KERN: PCI:   interrupt_line 00, interrupt_pin 00, min_grant 00, max_latency 00
KERN: PCI:   base reg 0: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 1: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 2: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 3: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 4: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 5: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: (not supported)
KERN: PCI: [dom 0, bus  0] bus   0, device 24, function  2: vendor 1022, device 1302, revision 00
KERN: PCI:   class_base 06, class_function 00, class_api 00
KERN: PCI:   vendor 1022: Advanced Micro Devices, Inc. [AMD]
KERN: PCI:   device 1302: Family 11h Processor DRAM Controller
KERN: PCI:   info: Bridge (Host bridge)
KERN: PCI:   line_size 00, latency 00, header_type 80, BIST 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size 00000000
KERN: PCI:   cardbus_CIS 00000000, subsystem_id 0000, subsystem_vendor_id 0000
KERN: PCI:   interrupt_line 00, interrupt_pin 00, min_grant 00, max_latency 00
KERN: PCI:   base reg 0: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 1: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 2: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 3: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 4: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 5: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: (not supported)
KERN: PCI: [dom 0, bus  0] bus   0, device 24, function  3: vendor 1022, device 1303, revision 00
KERN: PCI:   class_base 06, class_function 00, class_api 00
KERN: PCI:   vendor 1022: Advanced Micro Devices, Inc. [AMD]
KERN: PCI:   device 1303: Family 11h Processor Miscellaneous Control
KERN: PCI:   info: Bridge (Host bridge)
KERN: PCI:   line_size 00, latency 00, header_type 80, BIST 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size 00000000
KERN: PCI:   cardbus_CIS 00000000, subsystem_id 0000, subsystem_vendor_id 0000
KERN: PCI:   interrupt_line 00, interrupt_pin 00, min_grant 00, max_latency 00
KERN: PCI:   base reg 0: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 1: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 2: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 3: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 4: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 5: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: Secure Device
KERN: PCI: [dom 0, bus  0] bus   0, device 24, function  4: vendor 1022, device 1304, revision 00
KERN: PCI:   class_base 06, class_function 00, class_api 00
KERN: PCI:   vendor 1022: Advanced Micro Devices, Inc. [AMD]
KERN: PCI:   device 1304: Family 11h Processor Link Control
KERN: PCI:   info: Bridge (Host bridge)
KERN: PCI:   line_size 00, latency 00, header_type 80, BIST 00
KERN: PCI:   ROM base host 00000000, pci 00000000, size 00000000
KERN: PCI:   cardbus_CIS 00000000, subsystem_id 0000, subsystem_vendor_id 0000
KERN: PCI:   interrupt_line 00, interrupt_pin 00, min_grant 00, max_latency 00
KERN: PCI:   base reg 0: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 1: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 2: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 3: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 4: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   base reg 5: host 00000000, pci 00000000, size 00000000, flags 00
KERN: PCI:   Capabilities: (not supported)
KERN: ACPI: RSDP 0x00000000000F8120 000024 (v02 PTLTD )
KERN: ACPI: XSDT 0x00000000B7ECC915 000054 (v01 ACRSYS ACRPRDCT 06040000 INNA 00000000)
KERN: ACPI: FACP 0x00000000B7ED799C 0000F4 (v03 AMD    ANT      06040000 ATI  000F4240)
KERN: ACPI: DSDT 0x00000000B7ECC969 00B033 (v01 ATI    SB700    06040000 MSFT 03000001)
KERN: ACPI: FACS 0x00000000B7ED9FC0 000040
KERN: ACPI: SLIC 0x00000000B7ED7B04 000176 (v01 ACRSYS ACRPRDCT 06040000 ANNI 00000001)
KERN: ACPI: SSDT 0x00000000B7ED7C7A 0002B4 (v01 PTLTD  POWERNOW 06040000  LTP 00000001)
KERN: ACPI: APIC 0x00000000B7ED7F2E 00005E (v01 PTLTD  ? APIC   06040000  LTP 00000000)
KERN: ACPI: MCFG 0x00000000B7ED7F8C 00003C (v01 PTLTD    MCFG   06040000  LTP 00000000)
KERN: ACPI: HPET 0x00000000B7ED7FC8 000038 (v01 PTLTD  HPETTBL  06040000  LTP 00000001)
KERN: ACPI: Forced DSDT copy: length 0x0B033 copied locally, original unmapped
KERN: ACPI: 2 ACPI AML tables successfully acquired and loaded
KERN: ACPI: Dynamic OEM Table Load:
KERN: ACPI: OEMN 0xFFFFFFFF8209FA00 00020A (v01 AMD    NAHP     00000001 MSFT 03000001)
KERN: ACPI: Enabled 4 GPEs in block 00 to 1F
KERN: found io-apic with address 0xfec00000, global interrupt base 0, apic-id 2
KERN: mapping io-apic 0 at physical address 0xfec00000
KERN: io-apic 0 has range 0-23, 24 entries, version 0x00178021, apic-id 2
KERN: setting ACPI interrupt model to APIC
KERN: IRQ routing table with 13 entries
KERN: address 0x4ffff; pin 0; GSI 16; pci 0:4 pin 1 func mask 1; bios irq: 10; gsi 16; config 0x06
KERN: address 0x6ffff; pin 0; GSI 18; pci 0:6 pin 1 func mask 1; bios irq: 11; gsi 18; config 0x06
KERN: address 0x7ffff; pin 0; GSI 19; pci 0:7 pin 1 func mask 1; bios irq: 11; gsi 19; config 0x06
KERN: address 0x11ffff; pin 0; GSI 22; pci 0:17 pin 1 func mask 1; bios irq: 11; gsi 22; config 0x06
KERN: address 0x12ffff; pin 0; GSI 16; pci 0:18 pin 1 func mask 3; bios irq: 10; gsi 16; config 0x06
KERN: address 0x12ffff; pin 1; GSI 17; pci 0:18 pin 2 func mask 4; bios irq: 5; gsi 17; config 0x06
KERN: address 0x13ffff; pin 0; GSI 18; pci 0:19 pin 1 func mask 1; bios irq: 11; gsi 18; config 0x06
KERN: address 0x13ffff; pin 1; GSI 19; pci 0:19 pin 2 func mask 4; bios irq: 11; gsi 19; config 0x06
KERN: address 0x14ffff; pin 0; GSI 16; pci 0:20 pin 1 func mask 4; bios irq: 10; gsi 16; config 0x06
KERN: address 0xffff; pin 0; GSI 16; pci 3:0 pin 1 func mask 1; bios irq: 10; gsi 16; config 0x06
KERN: address 0xffff; pin 0; GSI 18; pci 9:0 pin 1 func mask 1; bios irq: 11; gsi 18; config 0x06
KERN: address 0x5ffff; pin 0; GSI 18; pci 1:5 pin 1 func mask 1; bios irq: 255; gsi 18; config 0x06
KERN: address 0x5ffff; pin 1; GSI 19; pci 1:5 pin 2 func mask 2; bios irq: 255; gsi 19; config 0x06
KERN: found interrupt override for bus 0, source irq 0, global irq 2, flags 0x0000KERN: 000f
KERN: free_io_interrupt_vectors: freeing 16 vectors starting from 0
KERN: reserve_io_interrupt_vectors: reserved 24 vectors starting from 0
KERN: using io-apics for interrupt routing
KERN: setting up apic for CPU 1: apic id 1, version 2147811344
KERN: CPU 1: logical apic id: 0x2
KERN: x86_init_fpu: CPU has SSE... enabling FXSR and XMM.
KERN: slab memory manager: created area 0xffffffff80801000 (238)
KERN: allocate_commpage_entry(3, 69) -> 0x0000000000000210
KERN: publish device: node 0xffffffff8217ac80, path acpi/namespace, module bus_managers/acpi/namespace/device_v1
KERN: registering power button
KERN: publish device: node 0xffffffff824a4330, path power/embedded_controller/0, module drivers/power/acpi_embedded_controller/device_v1
KERN: [33msdhci_pci:[0m supports_device(vid:1002 pid:4385)
KERN: usb xhci: no devices found
KERN: usb uhci: no devices found
KERN: usb ohci -1: iospace offset: 0xf0004000
KERN: usb ohci -1: successfully started the controller
KERN: usb ohci -1: iospace offset: 0xf0005000
KERN: usb ohci -1: successfully started the controller
KERN: usb ohci -1: iospace offset: 0xf0006000
KERN: usb ohci -1: successfully started the controller
KERN: usb ehci -1: disabling SB600/SB700 periodic list cache
KERN: usb ehci -1: successfully took ownership of the host controller
KERN: sitd entry size 128, itd entry size 128
KERN: usb ehci -1: successfully started the controller
KERN: usb ehci -1: disabling SB600/SB700 periodic list cache
KERN: usb ehci -1: successfully took ownership of the host controller
KERN: sitd entry size 128, itd entry size 128
KERN: usb ehci -1: successfully started the controller
KERN: usb hub 12: port 1: device removed
KERN: usb hub 22: port 1: new device connected
KERN: usb ehci 4: fullspeed device connected, giving up port ownership
KERN: usb hub 22: port 4: new device connected
KERN: get_boot_partitions(): boot volume message:
KERN: KMessage: buffer: 0xffffffff81b85238 (size/capacity: 347/347), flags: 0xa
KERN:   field: "booted from image" (BOOL): false
KERN:   field: "partition offset"  (LLNG): 32768 (0x8000)
KERN:   field: "packaged"          (BOOL): true
KERN:   field: "boot method"       (LONG): 0 (0x0)
KERN:   field: "boot drive number" (LLNG): 128 (0x80)
KERN:   field: "disk identifier"   (RAWT): data at 0xffffffff81b85344, 79 bytes
KERN: get_boot_partitions(): boot method type: 0
KERN: intel: ep_std_ops(0x1)
KERN: intel: ep_std_ops(0x2)
KERN: intel: pm_std_ops(0x1)
KERN: intel: pm_std_ops(0x2)
KERN: dos_std_ops()
Last message repeated 1 time
KERN: PCI-ATA: Controller in native mode: cmd 0x8420, ctrl 0x8416, irq 22
KERN: PCI-ATA: init channel...
KERN: PCI-ATA: channel index 0
KERN: PCI-ATA: bus master base 0x8400
KERN: PCI-ATA: init channel done
KERN: ata 0: _DevicePresent: device 0, presence 1
KERN: ata 0: _DevicePresent: device 1, presence 1
KERN: ata 0: deviceMask 3
KERN: ata 0: probing device 0
KERN: ata 0: signature of device 0: 0x0000
KERN: ata 0-0: model number: Hitachi HTS545032B9A300                 
KERN: ata 0-0: serial number: 090617PB5C00QDC1B7SG
KERN: ata 0-0: firmware rev.: PB3OC60F
KERN: ata 0-0: using DMA mode 0x16
KERN: ata 0: identified ATA device 0
KERN: ata 0: probing device 1
KERN: ata 0 error: device 1 failed, error code is 0x00
KERN: ata 0: signature of device 1: 0x0000
KERN: ata 0 error: device ready not set
KERN: ata 0-1 error: sending identify request failed
KERN: ata 0 error: command failed, error bit is set. status 0x51, error 0x04
KERN: publish device: node 0xffffffff824f8b68, path disk/ata/0/master/raw, module drivers/disk/scsi/scsi_disk/device_v1
KERN: ata 0-0 error: invalid target lun 1 for ATA device
KERN: ata 0-0 error: invalid target lun 2 for ATA device
KERN: ata 0-0 error: invalid target lun 3 for ATA device
KERN: ata 0-0 error: invalid target lun 4 for ATA device
KERN: ata 0-0 error: invalid target lun 5 for ATA device
KERN: ata 0-0 error: invalid target lun 6 for ATA device
KERN: ata 0-0 error: invalid target lun 7 for ATA device
KERN: ata 0 error: target device not present
KERN: ata 0 error: invalid target device
KERN: Last message repeated 12 times.
KERN: PCI-ATA: Controller in native mode: cmd 0x8418, ctrl 0x8412, irq 22
KERN: PCI-ATA: init channel...
KERN: PCI-ATA: channel index 1
KERN: PCI-ATA: bus master base 0x8408
KERN: PCI-ATA: init channel done
KERN: ata 1: _DevicePresent: device 0, presence 1
KERN: ata 1: _DevicePresent: device selection failed for device 1
KERN: ata 1: deviceMask 1
KERN: ata 1: probing device 0
KERN: ata 1: signature of device 0: 0xeb14
KERN: atapi 1-0: model number: TSSTcorp CDDVDW TS-L633B                
KERN: atapi 1-0: serial number:                     
KERN: atapi 1-0: firmware rev.: AC01    
KERN: atapi 1-0: using DMA mode 0x15
KERN: ata 1: identified ATAPI device 0
KERN: ata 1: ignoring device 1
KERN: publish device: node 0xffffffff824f8488, path disk/atapi/1/master/raw, module drivers/disk/scsi/scsi_cd/device_v1
KERN: atapi 1-0 error: invalid target lun 1
KERN: atapi 1-0 error: invalid target lun 2
KERN: atapi 1-0 error: invalid target lun 3
KERN: atapi 1-0 error: invalid target lun 4
KERN: atapi 1-0 error: invalid target lun 5
KERN: atapi 1-0 error: invalid target lun 6
KERN: atapi 1-0 error: invalid target lun 7
KERN: ata 1 error: target device not present
KERN: ata 1 error: invalid target device
KERN: Last message repeated 12 times.
KERN: periph_check_capacity: TRIM: Setting trim support to disabled
KERN: DMAResource@0xffffffff824f8ac8: low/high 0/100000000, max segment count 512, align 2, boundary 65536, max transfer 33553920, max segment size 33554432
KERN: slab memory manager: created area 0xffffffff8b001000 (621)
KERN: slab memory manager: created area 0xffffffff8b801000 (622)
KERN: periph_check_capacity: TRIM: Setting trim support to disabled
Last message repeated 1 time
KERN: intel: ep_std_ops(0x1)
KERN: intel: ep_std_ops(0x2)
KERN: intel: pm_std_ops(0x1)
KERN: intel: pm_identify_partition(0, 0: 0, 320072933376, 512)
KERN: btrfs [2165386:    16] invalid superblock!
KERN: [34mexfat:[0m invalid superblock!
KERN: [34mext2:[0m invalid superblock!
KERN: identify(0, 0xffffffff80f7ffa8)
KERN: ntfs: error: identify_partition: boot signature doesn't match
KERN: raw_command: 
KERN: dos_std_ops()
Last message repeated 1 time
KERN: intel: pm_scan_partition(0, 0: 0, 320072933376, 512)
KERN: intel: ep_std_ops(0x1)
KERN: intel: ep_identify_partition(0, 32768, 320072581120, 512)
KERN: intel: ep_std_ops(0x2)
KERN: intel: pm_identify_partition(0, 2: 32768, 320072581120, 512)
KERN: btrfs [2195318:    16] invalid superblock!
KERN: [34mexfat:[0m invalid superblock!
KERN: [34mext2:[0m invalid superblock!
KERN: identify(0, 0xffffffff80f7ff90)
KERN: ntfs: error: identify_partition: boot signature doesn't match
KERN: raw_command: 
KERN: dos_std_ops()
Last message repeated 1 time
KERN: device 0: /dev/disk/ata/0/master/raw
KERN:   media status:      No error
KERN:   device flags:      2
KERN:   offset:            0
KERN:   size:              320072933376 (305245.335 MB)
KERN:   content size:      320072933376
KERN:   block size:        512
KERN:   child count:       1
KERN:   index:             -1
KERN:   status:            0
KERN:   flags:             5
KERN:   volume:            -1
KERN:   disk system:       partitioning_systems/intel/map/v1
KERN:   name:              Hitachi HTS545032B9A300
KERN:   content name:      <NULL>
KERN:   type:              <NULL>
KERN:   content type:      Intel Partition Map
KERN:   params:            <NULL>
KERN:   content params:    <NULL>
KERN:   partition 2: /dev/disk/ata/0/master/0
KERN:     offset:            32768
KERN:     size:              320072581120 (305245 MB)
KERN:     content size:      320072581120
KERN:     block size:        2048
KERN:     child count:       0
KERN:     index:             0
KERN:     status:            0
KERN:     flags:             2
KERN:     volume:            -1
KERN:     disk system:       file_systems/bfs/v1
KERN:     name:              <NULL>
KERN:     content name:      Gateway
KERN:     type:              Be File System
KERN:     content type:      Be File System
KERN:     params:            type = 235 ; active = 0
KERN:     content params:    <NULL>
KERN: device 1: /dev/disk/atapi/1/master/raw
KERN:   media status:      No media present
KERN:   device flags:      5
KERN: Identified boot partition by partition offset.
KERN: periph_check_capacity: TRIM: Setting trim support to disabled
Last message repeated 1 time
KERN: bfs: mounted "Gateway" (root node at 524288, device = /dev/disk/ata/0/master/0)
KERN: Mounted boot partition: /dev/disk/ata/0/master/0
KERN: unknown [2286318:    16] Adding packages from "/boot/system/packages"
KERN: slab memory manager: created area 0xffffffff8c001000 (662)
KERN: usb hub 12: port 1: new device connected
KERN: usb hub 22: port 1: device removed
KERN: slab memory manager: created area 0xffffffff8c801000 (663)
KERN: slab memory manager: created area 0xffffffff8d001000 (664)
KERN: slab memory manager: created area 0xffffffff8d801000 (666)
KERN: slab memory manager: created area 0xffffffff8e001000 (668)
KERN: slab memory manager: created area 0xffffffff8e801000 (671)
KERN: slab memory manager: created area 0xffffffff8f001000 (672)
KERN: slab memoKERN: ry manager: created area 0xffffffff8f801000 (673)
KERN: slab memory manager: created area 0xffffffff90001000 (675)
KERN: slab memory manager: created area 0xffffffff90801000 (676)
KERN: slab memory manager: created area 0xffffffff91001000 (678)
KERN: slab memory manager: created area 0xffffffff91801000 (679)
KERN: slab memory manager: created area 0xffffffff92001000 (680)
KERN: unknown [22669380:    16] StringPool usage:
KERN: unknown [22669591:    16]   total unique strings:       92277,  1496906 bytes, overhead: 2122371 bytes
KERN: unknown [22669978:    16]   total strings with dups:   670946,  8355996 bytes
KERN: unknown [22670273:    16]   unshared strings:            3096
KERN: unknown [22670507:    16]   bytes saved:              4736719
KERN: unknown [22702939:    16] Adding packages from "/boot/home/config/packages"
KERN: unknown [22703610:    16] Failed to open packages activation file: No such file or directory
KERN: unknown [22703961:    16] Loading packages from activation file failed. Loading all packages in packages directory.
KERN: unknown [22721698:    16] StringPool usage:
KERN: unknown [22721874:    16]   total unique strings:       92277,  1496906 bytes, overhead: 2122371 bytes
KERN: unknown [22722262:    16]   total strings with dups:   670957,  8356061 bytes
KERN: unknown [22722556:    16]   unshared strings:            3094
KERN: unknown [22722791:    16]   bytes saved:              4736784
KERN: module: Search for file_cache/launch_speedup/v1 failed.
KERN: smbios_scan
KERN: found System Information at 0xffffffff820ca04d
KERN: found vendor 1 product 2
KERN: smbios_scan found vendor Gateway         product NV52 Series                    
KERN: publish device: node 0xffffffff91dd7ca0, path disk/virtual/ram/control, module drivers/disk/virtual/ram_disk/control/device_v1
KERN: loaded driver /boot/system/add-ons/kernel/drivers/dev/zero
KERN: usb_modeswitch: init_hardware()
KERN: usb_modeswitch: init_driver()
KERN: usb_modeswitch: trying module bus_managers/usb/v3
KERN: usb_modeswitch: publish_devices()
KERN: usb_modeswitch: uninit_driver()
KERN: loaded driver /boot/system/add-ons/kernel/drivers/dev/usb_modeswitch
KERN: loaded driver /boot/system/add-ons/kernel/drivers/dev/tty
KERN: loaded driver /boot/system/add-ons/kernel/drivers/dev/null
KERN: loaded driver /boot/system/add-ons/kernel/drivers/dev/dprintf
KERN: con_init: trying module console/frame_buffer/v1
KERN: loaded driver /boot/system/add-ons/kernel/drivers/dev/console
KERN: loaded driver /boot/system/add-ons/kernel/drivers/dev/disk/usb/usb_disk
KERN: allocate_commpage_entry(4, 16) -> 0x0000000000000258
KERN: no valid cpufreq module found
KERN: no valid cpuidle module found
KERN: set MTRRs to:
KERN:   mtrr:  0: base: 0xb7ec0000, size:    0x40000, type: 0
KERN:   mtrr:  1: base: 0xc0000000, size: 0x40000000, type: 0
KERN: set MTRRs to:
KERN:   mtrr:  0: base: 0xb7ec0000, size:    0x40000, type: 0
KERN:   mtrr:  1: base: 0xc0000000, size: 0x40000000, type: 0
KERN: kernel debugger extension "debugger/run_on_exit/v1": loaded
KERN: kernel debugger extension "debugger/usb_keyboard/v1": loaded
KERN: kernel debugger extension "debugger/invalidate_on_exit/v1": loaded
KERN: kernel debugger extension "debugger/hangm